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Confined Space Entry Permit Issuance And Atmospheric Testing
1.0 Form Objective & Regulatory Context
This Confined Space Entry Permit and Atmospheric Testing Log is designed to document the authorization and safe execution of confined space entries in industrial and manufacturing environments. It satisfies the requirements of WorkSafeBC Part 9 (Confined Spaces) and CSA Z1006 (Management of Work in Confined Spaces). The form ensures that all atmospheric hazards are identified, monitored, and controlled prior to and during entry, and that a formal permit is issued by a competent entry supervisor.
Use this form to record pre-entry atmospheric test results, continuous monitoring data, isolation verification, and emergency preparedness checks. It serves as a legal record of compliance and due diligence during confined space operations.
2.0 Administrative Details
Date of Entry: ____________________
Time of Entry (Start): ____________________
Time of Exit (End): ____________________
Entry Supervisor Name: ____________________
Confined Space Location/ID: ____________________
Purpose of Entry: ____________________
Permit Number: ____________________
Permit Valid Until (Date/Time): ____________________
3.0 Audit / Inspection Items
☐ Pass  ☐ Fail - Verify that the confined space has been isolated from all energy sources (lockout/tagout completed).
☐ Pass  ☐ Fail - Confirm that all hazardous energy sources (electrical, mechanical, pneumatic) are locked and tagged.
☐ Pass  ☐ Fail - Ensure that the atmosphere has been tested for oxygen content (acceptable range: 19.5% - 23.5%).
☐ Pass  ☐ Fail - Test for flammable gases/vapours (acceptable level: less than 10% of Lower Explosive Limit).
☐ Pass  ☐ Fail - Test for toxic gases (e.g., H2S, CO, VOCs) and record readings below applicable exposure limits.
☐ Pass  ☐ Fail - Verify that continuous atmospheric monitoring equipment is calibrated and functioning.
☐ Pass  ☐ Fail - Confirm that all entrants have been trained and are wearing appropriate PPE (harness, respirator, etc.).
☐ Pass  ☐ Fail - Ensure that a standby attendant is present and trained for rescue procedures.
☐ Pass  ☐ Fail - Verify that rescue equipment (tripod, winch, lifeline, first aid kit) is on site and inspected.
☐ Pass  ☐ Fail - Confirm that communication methods (radio, hand signals) are established and tested.
☐ Pass  ☐ Fail - Ensure that the entry permit is posted at the entrance of the confined space.
☐ Pass  ☐ Fail - Verify that all pre-entry checklists and test results are recorded and signed off.
4.0 Corrective Actions & Deficiencies
Issue Description: ________________________________________
Immediate Action Taken: ________________________________________
Corrective Action Required: ________________________________________
Assigned To: ________________________________________
Due Date: ________________________________________
Status (Open/Closed): ________________________________________
5.0 Sign-off & Authorization
Entry Supervisor Signature: __________________________ Date: ____________
Attendant Signature: __________________________ Date: ____________
Entrant Signature: __________________________ Date: ____________
Safety Manager Signature (if applicable): __________________________ Date: ____________

Regulatory Disclaimer: This audit log is a generic safety template. The end-user assumes all liability for validating all inspection parameters against WorkSafeBC, OH&S, and specific equipment manuals before active shop floor deployment.

	SafeDesk Digital Safety Management
	ryxen.ca






