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Hearing Conservation Program Noise Dosimetry Mapping Log
1.0 Form Objective & Regulatory Context
This Noise Dosimetry Mapping Log is designed to document and track noise exposure levels across designated work areas in industrial and manufacturing facilities. It satisfies the requirements of WorkSafeBC Part 7 (Noise Exposure) and CSA Z94.2-14 (Hearing Protection Devices – Selection, Care, and Use) by providing a systematic method for recording dosimetry readings, identifying high-noise zones, and supporting the Hearing Conservation Program.
Use this log to map noise levels at specific locations, record dosimeter serial numbers, note calibration status, and document any corrective actions taken when exposure limits are exceeded. All entries must be made by a qualified noise monitor or safety professional.
2.0 Administrative Details
Date of Survey: ____________________
Time of Survey (Start/End): ____________________
Inspector Name: ____________________
Inspector Title: ____________________
Facility Name: ____________________
Department/Area: ____________________
Weather Conditions (if applicable): ____________________
3.0 Audit / Inspection Items
☐ Pass  ☐ Fail - Verify dosimeter is calibrated per manufacturer specifications and within current calibration date.
☐ Pass  ☐ Fail - Record dosimeter make, model, and serial number.
☐ Pass  ☐ Fail - Identify and label each measurement location on a facility map or grid.
☐ Pass  ☐ Fail - Measure and record the Leq (equivalent continuous sound level) in dBA for each location.
☐ Pass  ☐ Fail - Measure and record the peak sound level (Lpeak) in dBC for each location.
☐ Pass  ☐ Fail - Note any dominant noise sources (e.g., machinery, ventilation, tools) at each location.
☐ Pass  ☐ Fail - Compare readings against WorkSafeBC action levels: 85 dBA Lex (daily noise exposure level) and 140 dBC peak.
☐ Pass  ☐ Fail - Document any hearing protection zone designations based on readings (e.g., mandatory HPD area).
☐ Pass  ☐ Fail - Record any employee observations or comments regarding noise exposure during the survey.
☐ Pass  ☐ Fail - Ensure all data is entered into the log within 24 hours of survey completion.
4.0 Corrective Actions & Deficiencies
Location ID / Grid Reference: ________________________________________
Measured Leq (dBA): ________________________________________
Measured Lpeak (dBC): ________________________________________
Issue Description (e.g., reading exceeds action level, missing signage): ________________________________________
Immediate Action Taken (e.g., issued hearing protection, posted warning sign): ________________________________________
Assigned To (name/title): ________________________________________
Target Completion Date: ________________________________________
Status (Open/In Progress/Closed): ________________________________________
5.0 Sign-off & Authorization
Noise Monitor / Inspector Signature: __________________________ Date: ____________
Safety Manager / Program Administrator Signature: __________________________ Date: ____________
Date of Sign-off: __________________________ Date: ____________

Regulatory Disclaimer: This audit log is a generic safety template. The end-user assumes all liability for validating all inspection parameters against WorkSafeBC, OH&S, and specific equipment manuals before active shop floor deployment.
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