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Machine Guarding Audit Checklist (ISO 12100)
1.0 Form Objective & Regulatory Context
This Machine Guarding Audit Checklist is designed to verify that all fixed, interlocked, and adjustable guards on industrial machinery comply with ISO 12100 (Safety of machinery — General principles for design — Risk assessment and risk reduction) and WorkSafeBC Part 12 (Guarding of Machinery). The checklist ensures that guards prevent access to hazardous moving parts, contain ejected materials, and do not create additional hazards. Use this form during routine inspections, after machine modifications, or as part of a scheduled safety audit.
2.0 Administrative Details
Date of Inspection: ____________________
Inspector Name: ____________________
Machine ID / Asset Number: ____________________
Machine Type / Model: ____________________
Department / Location: ____________________
Shift (Day / Afternoon / Night): ____________________
3.0 Audit / Inspection Items
☐ Pass  ☐ Fail - Fixed guards are securely fastened (bolts, welds, or equivalent) and cannot be removed without tools.
☐ Pass  ☐ Fail - Interlocked guards stop machine motion immediately when opened or removed.
☐ Pass  ☐ Fail - Adjustable guards (e.g., on saws or grinders) are set to the minimum opening required for the workpiece.
☐ Pass  ☐ Fail - Guards prevent access to pinch points, rotating shafts, belts, pulleys, and gears.
☐ Pass  ☐ Fail - No sharp edges, burrs, or protrusions on guards that could cause injury.
☐ Pass  ☐ Fail - Guards are made of durable material (e.g., steel, polycarbonate) appropriate for the hazard.
☐ Pass  ☐ Fail - Guards do not obstruct operator visibility of the work area unnecessarily.
☐ Pass  ☐ Fail - Emergency stop devices are accessible and functional (tested).
☐ Pass  ☐ Fail - Warning labels and lockout/tagout points are clearly visible and legible.
☐ Pass  ☐ Fail - Guards are free of damage, cracks, corrosion, or missing fasteners.
4.0 Corrective Actions & Deficiencies
Issue Description (e.g., guard missing, interlock bypassed): ________________________________________
Immediate Action Taken (e.g., machine locked out, guard replaced): ________________________________________
Assigned To (name of person responsible): ________________________________________
Target Completion Date: ________________________________________
Status (Open / In Progress / Closed): ________________________________________
5.0 Sign-off & Authorization
Inspector Signature: __________________________ Date: ____________
Supervisor / Manager Signature: __________________________ Date: ____________
Date of Sign-off: __________________________ Date: ____________

Regulatory Disclaimer: This audit log is a generic safety template. The end-user assumes all liability for validating all inspection parameters against WorkSafeBC, OH&S, and specific equipment manuals before active shop floor deployment.
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