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NFPA 25 Fire Sprinkler System Monthly/Annual Inspection Checklist
1.0 Form Objective & Regulatory Context
This inspection checklist is designed to document the monthly and annual inspection of fire sprinkler systems in accordance with NFPA 25: Standard for the Inspection, Testing, and Maintenance of Water-Based Fire Protection Systems. Compliance with this standard is required by WorkSafeBC regulations and local fire codes. The form ensures that all critical components are verified, deficiencies are recorded, and corrective actions are tracked to maintain system reliability and life safety.
2.0 Administrative Details
Date of Inspection: ____________________
Time of Inspection: ____________________
Inspector Name: ____________________
System Location / Building Name: ____________________
System Type (Wet/Dry/Pre-action/Deluge): ____________________
Inspection Type (Monthly / Annual): ____________________
3.0 Audit / Inspection Items
☐ Pass  ☐ Fail - Verify control valves are in the normal open position and sealed/locked.
☐ Pass  ☐ Fail - Check water flow alarm devices for proper operation (e.g., vane-type flow switch).
☐ Pass  ☐ Fail - Inspect all sprinkler heads for physical damage, corrosion, or obstructions.
☐ Pass  ☐ Fail - Verify that spare sprinkler heads are available in the required cabinet (per NFPA 25).
☐ Pass  ☐ Fail - Check pressure gauges on wet pipe systems for normal water pressure readings.
☐ Pass  ☐ Fail - Inspect dry pipe valves and ensure the system is properly charged with air pressure.
☐ Pass  ☐ Fail - Test the main drain valve and record static and residual pressure readings.
☐ Pass  ☐ Fail - Verify that all fire department connections (FDC) are accessible and caps are in place.
☐ Pass  ☐ Fail - Inspect pipe hangers and supports for signs of corrosion or loosening.
☐ Pass  ☐ Fail - Check that the system is free of leaks and that no unauthorized modifications exist.
☐ Pass  ☐ Fail - For annual inspection: test all control valves for full operation and record results.
☐ Pass  ☐ Fail - For annual inspection: perform a full flow test of the system (if required by local code).
4.0 Corrective Actions & Deficiencies
Deficiency Description: ________________________________________
Location of Deficiency: ________________________________________
Immediate Action Taken: ________________________________________
Corrective Action Required: ________________________________________
Assigned To: ________________________________________
Target Completion Date: ________________________________________
Status (Open / In Progress / Closed): ________________________________________
5.0 Sign-off & Authorization
Inspector Signature: __________________________ Date: ____________
Fire Safety Manager / Supervisor Signature: __________________________ Date: ____________
Date of Sign-off: __________________________ Date: ____________

Regulatory Disclaimer: This audit log is a generic safety template. The end-user assumes all liability for validating all inspection parameters against WorkSafeBC, OH&S, and specific equipment manuals before active shop floor deployment.
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