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Cooling Tower Daily Water Treatment And Conductivity Testing Log
1.0 Form Objective & Asset Scope
This daily log is used to track water treatment parameters and conductivity readings for the facility's cooling tower(s). Proper water chemistry control prevents scale formation, corrosion, and microbiological fouling, extending equipment life and maintaining heat transfer efficiency.
This log applies to all evaporative cooling towers, closed-circuit coolers, and associated recirculating water systems. Compliance with this log supports OEM warranty requirements and reduces unplanned downtime.
2.0 Administrative & Asset Details
Date: ____________________
Technician Name: ____________________
Cooling Tower ID / Asset Tag: ____________________
System Operating Hours (Hour Meter): ____________________
Ambient Temperature (°C): ____________________
Water Flow Rate (GPM / L/s): ____________________
3.0 Inspection / Parameter Checklist
☐ Pass  ☐ Fail - Visually inspect basin water for clarity, foam, oil sheen, or debris.
☐ Pass  ☐ Fail - Measure and record conductivity (µS/cm) using calibrated handheld meter.
☐ Pass  ☐ Fail - Measure and record pH level using calibrated probe or test strips.
☐ Pass  ☐ Fail - Measure and record water temperature at basin outlet (°C).
☐ Pass  ☐ Fail - Check chemical feed pump operation and verify chemical drum levels.
☐ Pass  ☐ Fail - Verify biocide residual (e.g., free chlorine, bromine, or non-oxidizing biocide) within target range.
☐ Pass  ☐ Fail - Inspect bleed/ blowdown valve operation and confirm proper cycling.
☐ Pass  ☐ Fail - Check make-up water meter reading and record totalizer value.
☐ Pass  ☐ Fail - Inspect drift eliminators for damage or blockage.
☐ Pass  ☐ Fail - Verify conductivity controller setpoint and alarm functionality.
☐ Pass  ☐ Fail - Record any water treatment chemical additions (type, amount, time).
☐ Pass  ☐ Fail - Check for visible leaks at pumps, valves, and tower basin.
4.0 Deficiencies & Work Order Generation
Issue Description: ________________________________________
Affected Component / Location: ________________________________________
Corrective Action Taken: ________________________________________
Parts Required: ________________________________________
Work Order Number (if created): ________________________________________
5.0 Sign-off & Return to Operations
Maintenance Technician Signature: __________________________ Date: ____________
Water Treatment Specialist Review (if applicable): __________________________ Date: ____________
Reliability Manager Review: __________________________ Date: ____________

Regulatory Disclaimer: This maintenance log is a generic template. The end-user assumes all liability for validating all inspection parameters, PM frequencies, and tolerances against specific OEM machinery manuals before active shop floor deployment.
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