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Industrial Air Compressor Preventive Maintenance Schedule Log
1.0 Form Objective & Asset Scope
This preventive maintenance log is designed to track the scheduled service of industrial air compressors (rotary screw and reciprocating types) used in manufacturing and facility operations. Proper compressor maintenance ensures reliable compressed air supply, reduces unplanned downtime, extends equipment life, and maintains energy efficiency. This log supports compliance with OEM service intervals and internal reliability standards.
2.0 Administrative & Asset Details
Date: ____________________
Technician Name: ____________________
Machine ID / Asset Tag: ____________________
Compressor Model: ____________________
Hour Meter Reading (Start): ____________________
Hour Meter Reading (End): ____________________
PM Interval (e.g., 250h / 500h / 1000h): ____________________
3.0 Inspection / Parameter Checklist
☐ Pass  ☐ Fail - Check compressor oil level and top up to full mark if required.
☐ Pass  ☐ Fail - Inspect oil filter condition and replace if due per interval.
☐ Pass  ☐ Fail - Inspect air filter element; clean or replace as needed.
☐ Pass  ☐ Fail - Check belt tension and alignment; adjust or replace if worn.
☐ Pass  ☐ Fail - Drain moisture from receiver tank and verify auto drain trap operation.
☐ Pass  ☐ Fail - Inspect all hoses and fittings for leaks, cracks, or abrasion.
☐ Pass  ☐ Fail - Verify safety relief valve is free and not leaking.
☐ Pass  ☐ Fail - Record discharge air temperature (should be within OEM range).
☐ Pass  ☐ Fail - Record system operating pressure and compare to setpoint.
☐ Pass  ☐ Fail - Test emergency stop button and automatic shutdown functions.
☐ Pass  ☐ Fail - Check for unusual vibration or noise during operation.
☐ Pass  ☐ Fail - Clean exterior of compressor and surrounding area of debris.
4.0 Deficiencies & Work Order Generation
Issue Description: ________________________________________
Parts Required: ________________________________________
Work Order Number: ________________________________________
Priority (Low / Medium / High / Critical): ________________________________________
Follow-up Action Required: ________________________________________
5.0 Sign-off & Return to Operations
Maintenance Technician Signature: __________________________ Date: ____________
Reliability Manager Review: __________________________ Date: ____________
Operations Supervisor Acknowledgment: __________________________ Date: ____________

Regulatory Disclaimer: This maintenance log is a generic template. The end-user assumes all liability for validating all inspection parameters, PM frequencies, and tolerances against specific OEM machinery manuals before active shop floor deployment.
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